Procedure to certify  
CFPA-E Fire Safety Specialists  
in Building Design

**CFPA-E Guideline No 40:2023 F**

Please add current image!



****

**The CFPA Europe develops and publishes common guidelines about fire safety, security, and natural hazards with the aim to achieve similar interpretation and to give examples of acceptable solutions, concepts, and models. The aim is to facilitate and support fire protection, security, and protection against natural hazards across Europe, and the whole world.**

**Today fire safety, security and protection against natural hazards form an integral part of a modern strategy for survival, sustainability, and competitiveness. Therefore, the market imposes new demands for quality.**

**These Guidelines are intended for all interested parties and the public. Interested parties includes plant owners, insurers, rescue services, consultants, safety companies and the like so that, in the course of their work, they may be able to help manage risk in society.**

**The Guidelines reflect best practice developed by the national members of CFPA Europe. Where these Guidelines and national requirements conflict, national requirements shall apply.**

**This Guideline has been compiled by the Guidelines Commission in association with the Training Commission and is adopted by the members of CFPA Europe.**

**More information:** [**www.cfpa-e.eu**](http://www.cfpa-e.eu)



Zurich, October 2023 Cologne, October 2023  
CFPA Europe Guidelines Commission

Elisabetta Carrea Hardy Rusch  
Chairman Chairman



**Contents**

[1 Introduction 4](#_Toc150247276)

[2 Scope 4](#_Toc150247277)

[3 Definitions 5](#_Toc150247278)

[4 Requirements to be eligible as CFPA-E Fire Safety Specialist in Building Design 5](#_Toc150247279)

[4.1 Education 5](#_Toc150247280)

[4.2 Specific Training 6](#_Toc150247281)

[4.3 Requirements to be a candidate for examination 6](#_Toc150247282)

[5 Recommended curriculum content for a Fire Safety Specialist in Building Design 8](#_Toc150247283)

[5.1 Core topics of expertise 9](#_Toc150247284)

[5.2 Additional “Application focused” topics 10](#_Toc150247285)

[6 Certification Procedure 12](#_Toc150247286)

[6.1 Eligibility 12](#_Toc150247287)

[6.2 Examination 12](#_Toc150247288)

[6.2.1 Practical case 12](#_Toc150247289)

[6.2.2 Battery of questions 13](#_Toc150247290)

[6.3 Certification 14](#_Toc150247291)

[6.4 Certificate validity 14](#_Toc150247292)

[6.5 Skills maintenance 14](#_Toc150247293)

[7 CFPA-E Courses related to Fire Safe Building Design 16](#_Toc150247294)

[7.1 CFPA-E Courses 16](#_Toc150247295)

[7.2 CFPA-E Courses & Guidelines for “Application focused” topics 17](#_Toc150247296)

[8 Quality and Independency 19](#_Toc150247297)

[8.1 Internal Audits 19](#_Toc150247298)

[8.2 Independency 19](#_Toc150247299)

[European guidelines 20](#_Toc150247300)

Key words: Fire Safety, Building Design, Fire Safety Specialist, Certification

# Introduction

The field of fire protection in building design has developed t throughout the world, including Europe. Due to its basis in science, the areas in which fire prevention knowledge could potentially be applied are many, but at present application of this knowledge is limited. There are gaps regarding fire and its possible interactions with the building environment and occupants.

As an alternative to conventional methods, such as prescriptive code application, fire safety design methods are often applied to provide a holistic fire safety concept that specifically adapts to the environmental conditions and hazard of any building like a tailored suit. This approach is particularly useful for innovative designed buildings, where the conditions are not adequately covered by prescriptive building regulations.

The application and acceptance of fire safe building design differs between the various European countries. Few countries have requirements for qualification of practitioners (for example, a university degree or a diploma in Fire Protection Engineering). In many countries, there are still limitations to the application of these methods. In some countries a performance-based approach must be accepted by authorities on national, regional or local level

In all the processes involved on a site up to when the fire protection concept is implemented on site, the designer plays a very important role, and should be able to demonstrate knowledge of the principles of engineering that are to be applied in this case. This guideline “Procedure to Certify CFPA-E Fire Safety Specialists in Building Design” describes the minimum qualification requirements for a specialist to be considered by the CFPA-E for certification as a CFPA-E Fire Safety Specialist in the field of Building Design.

This guideline forms the basis for the CFPA Europe to recognise the knowledge of an individual, by obtaining the status of a “CFPA-E Fire Safety Specialist in Building Design”. National requirements for Fire Safety Specialists in this field shall be considered. By obtaining the status of “CFPA-E Fire Safety Specialist in Building Design”, CFPA-E endorses the knowledge and experience of a certain individual having this status, but this status brings no legal competency without fulfilling the national requirements of each country.

# Scope

There is a need for European recognized diplomas and a European approach to accreditation and registration or certification of fire safety specialists in building design and other fire safety practitioners in Europe. The approach needs to be based on established levels of competency appropriate to their roles. Qualification of practitioners has been identified by several organizations as an important part of the professional recognition of fire safety engineers worldwide.

This Guideline presents a comprehensive procedure to qualify and recognize the knowledge and experience of a Fire Safety Specialist in Building Design as defined in Section 3, with the curriculum and competencies described in Section 5. The procedure is developed, supported and recognized by the CFPA-E and its member Associations.

# Definitions

**Fire Safety:** Condition of built environment, where the individually existing fire hazards and risks to persons and the environment are reduced to an acceptable or tolerable level thereby meeting the fire safety objectives and functional requirements as outlined in building codes, regulations or insurer or building owner requirements.

The fire protection measures are intended for the fire prevention and limitation of fire and smoke propagation in the event of fire to achieve the necessary fire safety and to fulfil the additional interests of building owner and user, e.g. conservation of property, limitation of business interruption and another subsequent damage. Fire protection systems can also contribute to the preservation of life. Thus, some fire protection systems are compulsory by law.

**Fire Safe Building Design:** Procedures, which are based on scientific principles, and their application to the determination of physical characteristics of a fire in the built environment and its impact regarding fire safety, e.g. development of the temperature propagation of fire and smoke. Protection methods can be taken into account in the design parameters of a fire safe building. Protection methods include the design of passive and active systems that fulfil the fire safety objectives. The design procedure may rely on installation rules, calculation procedures, experimental evaluations and operational arrangements.

**CFPA-E Fire Safety Specialist in Building Design (CFPA-E BDS):** A person who has successfully demonstrated knowledge, skills and experience in Fire Safe Building Design in terms of the criteria outlined in this document.

**CFPA-E Examination Committee:** Entity composed of voluntary members from the CFPA-E Association. The committee will prepare the wording of the examination, and will submit it to every member country of CFPA-E association willing to implement the certification procedure in its country.

**National Examination Board:** In every member country willing to implement this certification procedure, the local CFPA-E Association will appoint suitable persons to the Examination Board, which will evaluate applicants in terms of the competency requirements outlined in this document. The examination board will be composed of at least 3 members from different fields related to fire safety (for example, fire brigades, insurers, consultants, construction companies). It´s up to every national Association to decide the components of the board in that country.

# Requirements to be eligible as CFPA-E Fire Safety Specialist in Building Design

## Education

The title of CFPA-E Fire Safety Specialist in Building Design (hereafter CFPA-E BDS) can be awarded to any candidate with a **proportional balance of education and experience**; and who has successfully passed an examination attesting to that level of education and experience.

The curriculum needs to have a good foundation of mathematics, physics, chemistry and engineering practice. These feed into good skills in fluid mechanics, thermodynamics, heat transfer, etc, which in turn underpins fire dynamics and the understanding of fire and smoke spread which is fundamental for the knowledge of fire safe building design.

Candidates with the following educational background are eligible to apply for CFPA-E BDS registration:

* Master’s degree (at least 4 years) in Fire Safety related discipline from an accredited college or university. These programs are geared toward the development of theoretical skills, and consist of a sequence of courses on fire safety fundamentals and design, built on a foundation of physics, mathematics and science courses.
* Bachelor’s degree (at least 3 years) in Fire Safety related discipline from an accredited college or university. These programs are oriented toward application, and provide their students the basics in physics, mathematics and science courses.

To be eligible as a CFPA-E BDS candidate, the background education must include specific subject matter as specified in the next subchapter.

In every case, candidates will also have to demonstrate professional experience in the field of fire safety.

## Specific Training

CFPA-E offers specific training modules in fire safety throughout Europe. In addition, some colleges and universities offer programs and individual courses in topics related to fire protection engineering.

In fire safety, as in other scientific disciplines, experience is required to become a specialist. Experience can also be a good supplement of specific training courses in a certain field.

Every candidate must have completed the education and specific training with professional experience. The years of experience needed to be eligible will be different depending on the education and training base of each candidate.

Experience shall include the project-related use of specific design tools, for example (not an exhaustive list):

* Quantitative and qualitative risk analysis methods.
* Hydraulic calculation software.
* Calculation of Fire performance of structures.
* Fluid dynamic design tools.
* Smoke extraction calculation.
* Evacuation modelling software.
* Fire and Smoke modelling software.

## Requirements to be a candidate for examination

The candidates to the examination as CFPA-E BDS must demonstrate that they fulfil the requirements stated in the next subchapters regarding Education, Specific training, and Professional Experience.

Candidates must attain at least 50 points to be eligible for examination. A minimum of 10 points in each of the categories are needed.

|  |  |  |  |
| --- | --- | --- | --- |
| **CATEGORY** | **CRITERIA** | **POINTS** | **ACCEPTABLE DOCUMENTATION** |
| EDUCATION | Master (at least 4 years) in Engineering (other than Fire Engineering), Architecture, Applied Physics or similar disciplines. | 20 | Diploma copy |
| Bachelor’s degree (at least 3 years) in Fire Safety Disciplines | 20 |
| Bachelor’s degree (at least 3 years) in Engineering (other than Fire Safety Disciplines), Architecture, Applied Physics or similar disciplines. | 10 |
| Master (at least 4 years) in other disciplines and at least 60 ECTS credits in Fire Safety related disciplines | 20 |
|  | Bachelor’s degree (at least 3 years) in other disciplines and at least 60 ECTS credits in Fire Safety related disciplines | 10 |  |
| TRAINING | CFPA-E Basic Fire Safety Engineer Training Program as described in section 7.1 | Max. 20 | Certificate or Diploma (including examination) |
| CFPA-E Application-Focused Fire Protection courses as described in section 7.2 | Max. 10 |
| Other Fire Safety courses (1 point/ 30h course) | Max. 10 |
| PROFESSIONAL EXPERIENCE | Project Director (10 points/year) | Unlimited \* | Fire Safety Engineering Design Brief (FEDB) or;  Curriculum Vitae and list of references witnessed by at least two persons working in the field of fire safety |
| Responsible for one area in the project (5 points/year) | Unlimited \* |

Table 1. Requirements to be a candidate for examination to CFPA-E BDS

Education degrees shall be documented through a diploma copy issued by the University or College, specifying the degree obtained and duration.

Training shall be documented through a certificate or diploma, issued by the course organizer. The course must include an examination on the training topics to check the course has been profitable for the student.

Professional experience shall be demonstrated by the presentation of a Fire Safety Engineering Design Brief (FEDB) of the project, with the following minimum content:

* Project Scope. Define scope/extent of fire safety engineering works e.g. new construction of a building, additions and alterations to partial building or whole building or renovation of an existing building for a change of use.
* Structure of the project; responsibility areas.
* Applicant’s area of responsibility within the project.
* Duration of the project.
* Safety objectives and Acceptance criteria.
* Building characteristics: Description, proximity to neighbouring buildings, number of floors and general layout.
* Occupant characteristics: Occupant load, physical attributes, awareness level…
* Choice of Fire Scenarios: Describe the plausible fire scenarios considered, why they were used and identify the ‘worst credible’ fire scenario.
* Design parameters: Identify and select design parameters, e.g. design fire, design occupant groups.
* Method of evaluation. The evaluation should include description of the analysis method and the design tools used; any computational tools used should be discussed along with the input and output.
* Assumptions and Limitations.
* Conclusions.

The candidate will also present a responsible declaration indicating how much time was directly involved in the project.

In the case of FEDB being unavailable, experience shall be demonstrated by a Curriculum Vitae witnessed by two persons working in the field of fire safety or building design. The applicant and the witnesses shall not be related to each other. In addition to the CV, the applicant shall provide a list of references, with approximations on time spent on the project and the contents of the applicant’s attribution to the project in detail. The list of references shall also be witnessed, to be true by two persons working in the field of fire safety or building design.

# Recommended curriculum content for a Fire Safety Specialist in Building Design

The field of fire safe building design can be described as broad and deep. Design issues can require many levels of understanding, ranging from the qualitative understanding, to the simple calculation, the zone model and eventually CFD implementation.

The problem is that with each increasing level of complexity, the breadth of knowledge required to deliver that complexity increases. For example, only a little knowledge is required to have a qualitative understanding of smoke control. To carry out simple calculations, a knowledge of mathematics is required as well. To use a zone model requires a person to spend time learning how to use the model, and to know its limitations. To use CFD to work out a smoke control problem, even more skill is required while still keeping the depth of knowledge to implement proper scenarios. Finally, to make a fire safety approach, interactions between smoke control and extinguishing systems, detection and alarm systems, and egress time, must be carefully considered and implemented in the fire scenario.

In summary, there is a limit to the amount of knowledge which one person can have. A person’s knowledge can be broad but shallow or it can be narrow but deep. It would be difficult to find any individual whose knowledge was both, broad and deep.

For these reasons, it is necessary to state a minimum level of fundamental knowledge and competence for a Fire Safety Specialist in Building Design. This minimum level is composed of core topics that the Specialist has to understand and demonstrate adequately. In a second stage, the Specialist can specialize and focus on certain topics.

The following chapters describe the core expertise topics and the additional “application focused” topics or courses. These topics generally agree with the definitions of skills and competences that constitutes a Fire Safety Specialist in Building Design. A similar approach has been defined by the Society of Fire Protection Engineers (SFPE) in their “White Paper for Professional Recognition for Fire Safety Engineering”.

## Core topics of expertise

**Fire Dynamics and Fire Chemistry**

The objective is to understand the various stages of fire, to provide a knowledge base concerning the different methods and techniques applied in the analysis of a fire sequence and develop ability to critically examine those methods in terms of practical application. Fire Chemistry may be taught within a Fire Dynamics course to provide further background knowledge regarding combustion reactions and heat transport. Collectively, information should increase design-related skills.

**Fire Risk/Hazard Analysis**

The objective is to provide knowledge in the areas of probability and statistics, of the concepts, tools and methods of hazard assessment and risk analysis, and of the use and application of these in fire related scenarios. A general understanding of how fire affects people (including egress), property and society as a whole should be provided.

**Performance-Based Design**

The objective is to provide knowledge regarding development of fire safety engineering solutions from first principles to achieve fire performance objectives. This requires skills developed from previous fundamental fire safety engineering coursework. Various levels of design and consequences should be discussed as well as the specification of all key parameters that are the basis for the performance-based design.

**Building Fire Safety**

The objective is to provide a general understanding of building fire protection, code and standard concerns, and may include fundamental concepts of equivalencies and/or Performance Based Design.

**Fire Protection Measures**

The objective is to provide a general understanding of fire mitigation, including structural fire protection; mechanisms of escape and alarm system; water and non-water based suppression; detection systems; smoke and heat exhaust ventilation systems; general possible interactions of different fire protection measurements; fire modelling; fire testing and code and standard concerns.

## Additional “Application focused” topics

**Fire Modelling**

The objective is to provide knowledge of zone and field (CFD) models, including the technical basis for enclosure fire model elements, the limitations of computer-based fire models and the use of current computer-based fire models for practical FSE problems.

**Fire Testing**

The objective is to provide knowledge of test scenario, apparatus, methodologies, processes and data analysis related to fire hazards, assessment methods of fire characteristics of building materials and structures for engineering and research. It is also important that the CFSE knows the background and limits of fire tests.

**Water-Based Suppression**

The objective is to provide knowledge of fundamental principles, design criteria and installation requirements for water-based and foam water fire suppression systems, including, classification of occupancy hazards in order to establish the proper sprinkler design criteria, the design of sprinkler and water mist systems for the specific construction features and occupancy involved, and the effects of various forms of heat transfer and oxygen displacement characteristics relating to water-based suppression.

**Special Hazards – Non water-based suppression**

The objective is to provide knowledge of fundamental principles, design criteria and installation requirements for non-water based fire suppression (including halon, carbon dioxide, inert gas, halocarbon agents, and dry chemical) used in different types of application (deluge, and local applications.

**Detection, Alarm & Smoke control Systems**

The objective is to provide knowledge of fundamental principles, design criteria and installation requirements for fire detection, occupant notification and smoke control systems, including how to analyze, evaluate, and specify these systems.

**Explosion Prevention & Protection**

The objective is to provide basic knowledge related to deflagrations and detonations and methods used to prevent ignition and limit the effects of deflagrations, including explosion suppression systems and pressure resistant & pressure relieving construction; BLEVE theory and prevention.

**Structural Fire Protection**

The objective is to provide knowledge regarding the impact of fire exposure on materials used in construction assemblies, the role various construction features play in the fire resistance of the assembly and the application of mechanics and heat transfer engineering principles. Computer based analysis of structures exposed to fire.

**Fire Investigation**

The objective is to provide knowledge of fire investigation with regard to gathering and interpreting fire scene evidence; utilizing laboratory forensic testing; researching related codes, standards & technical reports and re-construction of the fire scenario with physical and numerical models.

**Fire Protection Related Codes & Standards**

The objective is to provide knowledge of the use and application of building codes and related reference standards, including both active and passive fire protection, people evacuation, interaction between systems.

**Egress and Life Safety Analysis**

The objective is to provide knowledge of human behaviour in fire, including physiological and psychological response, decision-making and movement and of approaches, tools and methods to integrate this knowledge with knowledge gained from other courses to evaluate life safety issues in the event of fire. While a basic knowledge may be provided within several other separate courses, focused applications level course work is helpful for those students that will design egress systems, including special situations using performance-based designs with complicated occupancies that potentially modify human behaviour.

**Storage & Transportation of Hazardous Materials**

The objective is to provide knowledge of the handling, transportation and storage of hazardous materials including limitations of amounts stored, determination of required separation distances and proper identification. Such information may be of particular interest to those that work in public service or are responsible for public transportation of such materials.

**Management of Wildland-Urban interface Fires**

The objective is to provide knowledge regarding technological, economic, social and political issues affecting fire management in the interface of rural and urban areas. Includes related codes and standards, fire risk analysis, evacuation and incident response planning.

**Industrial Fire Safety**

The objective is to use principles of fire dynamics, heat transfer and thermodynamics are combined with a general knowledge of automatic detection and suppression systems to analyze fire protection requirements for generic industrial hazards. Topics covered include safe separation distances, plant layout, hazard isolation, smoke control, warehouse storage, and flammable liquid processing and storage. Historic industrial fires influencing current practice on these topics can also be discussed.

**Consequence Analysis**

The objective is to provide an introduction to the field of Consequence Estimations, within the fire safe building design operational field. It will also form a valuable complement to the course, Fire Risk Analysis, insofar as the consequences of undesirable leakages of gases and liquids are concerned.

**Risk Based Land Use Planning**

The objective is to provide the applicant with sufficient knowledge to allow collaboration at early stages in the planning process so that risk analyses can be included and used to create a base at a strategic stage of the planning work where the objective is a robust and sustainable society.

# Certification Procedure

## Eligibility

The candidates to the examination as CFPA-E BDS must demonstrate that they fulfil the requirements stated in Section 4 ”Requirements” to be a candidate for examination”. The supporting documents are to be submitted to the CFPA-E member association in the country where the applicant wishes to do the exam. All the documentation must be sent in the official local language of the country or in English.

The National Examination board will study the documents and decide how many points can be achieved by the applicant. Where the applicant obtains the minimum number of points to be eligible, they will be permitted to undertake the competence evaluation.

## Examination

All the candidates must pass a competency exam to demonstrate their competence as Fire Safety Specialist in Building Design. The examination will be offered by the CFPA-E member association in each country. The examination requirements and standards will be similar level in all countries. To ensure this, an CFPA-E Examination Committee will develop the contents of the exam. The CFPA-E Examination Committee will be composed of voluntary members of the CFPA-E associations that are willing to implement the certification process.

The exam will have two parts, a practical case for designing the adequate fire safety measures, and a battery of questions related to different aspects of fire safe building design.

### Practical case

The wording of the case will provide information about the functionality and activities carried out in the building: construction, occupancies, occupants’ characteristics, etc.

The National Examination Board is responsible for implementing and evaluating the practical case based on the implementation and evaluation practices established by the CFPA-E Examination committee. The practical case must cover the applications of the principles of fire safety engineering including the approach and development of the fire safety concept for a certain building or industry. As an example, some of the objectives of the practical case can be: Ensuring a safe evacuation, guarantee the continuity of activity, contain the fire smoke in a limited area, avoid the collapse of the building structure under a fire condition, etc.

The candidate will apply a technical base to make the safety approach: prescriptive or voluntary design codes, technical publications, engineering handbooks, and in general, every document that can be used to justify the validity of the solution proposed. If some calculations are needed to prove the performance of the solution, they shall be included in the dossier. For those requirements that cannot be fulfilled under a prescriptive design method, the applicant will develop a solution based on the application of a Performance Based Design method that will provide at least an equivalent fire safety level. The safety approach is based on the procedure described in the SFPE Engineering Guide to Performance-Based Fire Protection. The candidate will have two months to study the case and make a fire protection approach.

The proposal with the Fire Safety approach will be submitted to the local CFPA-E member association, where an Examination Board will evaluate the solution. The candidate will be summoned to describe and defend his proposal in front of this Examination Board. The Board will ask the applicant specific questions about the design, and will ask him for a new approach in case some of the acceptance parameters are changed. The Examination Board will also be able to ask the candidate during examination on how to make a basic fire safety approach for the fulfilment of any of the safety objectives that have not been developed.

The candidate must be able to describe clearly in his proposal:

**Fire safety objectives:**

The objectives of fire safety and protection design shall be clearly defined. These objectives are generally quite broad and deal with life safety, property protection, business interruption and environment preservation.

**Functional requirements:**

The objectives are very broad but they are not sufficiently specific to provide a basis for an engineering design. It is therefore essential to stablish functional requirements associated with performance criteria that can be used to assess whether the fire safety objectives have been adequately achieved.

**Qualitative design review:**

The qualitative design review includes:

* The definition of acceptance criteria.
* The risk analysis and selection of fire scenarios.
* The initial proposal of fire safety and protection design.

Prior to carrying out fire engineering calculations, it is necessary to set certain criteria, which results must meet before they will be considered sufficiently close to reality to be acceptable. These criteria are called “acceptance criteria”.

The candidate must then select the most likely or hazardous fire scenarios, according to a previous risk analysis.

According to the results of the corresponding fire scenario, the candidate will propose the fire safety and protection solutions, which will limit the frequency and the consequence of the fire.

**Quantitative analysis of design:**

This quantitative analysis of design involves the determination of the consequences of the design fires (fire scenarios) considering the proposed fire safety solutions. Engineering methods are used to evaluate the potential solutions.

**Fire protection systems:**

The candidate will be able to make a basic design of the fire protection systems proposed in each zone, for both active and passive fire protection systems.

### Battery of questions

The candidate shall answer a battery of 20 short questions regarding different fire protection and fire safety aspects related to the “Application focused topics” described in Section 5.2.

The CFPA Examination Committee will decide how many questions will be related to each topic. The Examination Board in every country will decide the wording of every question. The battery of questions will include some regarding to local (national) regulations.

## Certification

Where the applicant succeeds in passing both tests, and has paid the examination fee, the candidate will be awarded with a certificate that grants accredits him as a CFPA-E Fire Safety Specialist in Building Design.

Where the applicant fails one of the two tests, the candidate will be permitted to repeat only the test failed in the next call for examination, by paying the examination fee for that specific test. Where the applicant fails again and remains interested in obtaining the certificate, full re-examination will be required.

## Certificate validity

The certificate is valid for a period of 5 years. After the end of each period, the certificate can be renewed provided that:

* The applicant has paid the renewal fee to the entity that issued the certificate.
* The applicant has demonstrated that he/she is involved in a Continual Professional Development process that enables knowledge and skills in fire safety to be maintained. Certification is evaluated according to a scoring system that includes credits for working experience, for continuous training programs, and for attending conferences. See chapter 6.5 to see how to demonstrate skills maintenance.

In case the certificate´s period of validity expires and the applicant has not been able to demonstrate skills maintenance according to 6.5, the only possible way to obtain the certification is by passing the exam again. The applicant may re-validate an expired certificate within one year of the expiration date.

## Skills maintenance

To renew the certification, the applicant must accumulate at least 30 points in different activities related to fire protection, during the 5 years cycle between recertification. As the fire safety specialist must keep his knowledge up-to-date, at least 3 points will have to come from professional development activities:

|  |  |  |  |
| --- | --- | --- | --- |
| **CATEGORY** | **ASSIGNED POINTS** | **MAX. PERMITTED POINTS** | **ACCEPTABLE DOCUMENTATION** |
| Professional practice | Project Director (1 point/dedicated month) | 27 points per cycle | Fire Engineering Design Brief (FEDB) (1) or;  list of references witnessed by at least two persons working in the field of fire safety or building design |
| Responsible for one area in the project (0,5 points/dedicated month) | 25 points per cycle |
| Professional development – CFPA-E courses | 3 points per course and day or equivalent (2) | 25 points per cycle | Attestation of participation |
| Professional development – other fire protection courses | 1,5 points per course and day (3) | 15 points per cycle | Attestation of participation |
| Professional development – fire protection conferences | 1 points per conference day or equivalent (5) | 15 points per cycle | Attestation of participation |
| (1) Fire Engineering Design Brief to demonstrate professional practice will have the minimum contents described in Section 4.4.  (2) 1 day = At least 6h of effective training or course = 3 points. See Tables 3 & 4.  (3) 1 day = At least 6h of effective training or course = 1,5 points  (4) 1 day = At least 6h of effective conference = 1 point  (5) 1 day = At least 6h of effective conference = 0,5 points | | | |

Table 2. Requirements for recertification of CFPA-E BDS

For re-certification, to justify “Training” requirements (attendance to courses and conferences) will be enough to present an attestation of participation (no need for examination).

# CFPA-E Courses related to Fire Safe Building Design

## CFPA-E Courses

The following table describes which CFPA-E Courses deal with the core topics as detailed in section 5.1.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Core Topic | | CFPA-E Course | Duration (hours/ credits) | Points for certification\* | Points for recertification \*\* |
| Fire Dynamics and Fire Chemistry  Building Fire Safety  Fire Protection Systems | | Fire Safety – Management Cycle | 60 | 5,0 | 27 |
| Fire Safety – Technical Cycle | 90 | 7,5 | 27 |
| Fire Risk/Hazard Analysis | | Fire Risk Management | 30 | 2,5 | 15 |
| Fire Risk Assessment | 30 | 2,5 | 15 |
| Performance Based Design | | Performance Based Design for Fire Safety | 90 | 7,5 | 27 |
| Principles of fire safety engineering | 30 | 2,5 | 15 |
|  | \* Related to Table 1  \*\* Related to Table 2 | | | | |

Table 3. CFPA-E Courses for Core FSE Topics

## CFPA-E Courses & Guidelines for “Application focused” topics

The following table describes which CFPA-E Courses deal with the additional “application focused” FSE topics as detailed in section 5.2. These courses complement the basic competences of a FSE by specialization in certain topics.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Application Focus Topics | Related CFPA-E Courses | Duration (hours/ credits) | Points for certification\* | Points for recertification \*\* | Related CFPA-E Guidelines |
| Water-Based Suppression systems | Sprinkler operator | 12 | 0,5 | 6 | -- |
| Sprinkler system: basic course | 12 | 0,5 | 6 | -- |
| Non water-based suppression (special hazards) | Gas system operator | 12 | 0,5 | 6 | No.14:  Fire protection in information technology facilities |
| Operator of Stationary Fire Protection Systems containing Fluorinated Greenhouse Gases | 12 | 0,5 | 6 |
| Detection, Alarm, & Smoke Control Systems | Fire Detection and Alarm Systems Operator | 6 | 0,5 | 3 | -- |
| Smoke and heat Exhaust Systems Operator | 6 | 0,5 | 3 |
| Explosion Prevention & Protection | Explosion protection manager | 30 | 2,5 | 15 | No.31:  Protection against self-ignition and explosions in handling and storage of silage and fodder in farms |
| Explosion (Prevention and Protection in places where explosive atmospheres may occur) | 12 | 1,0 | 6 |
| Classification of explosive Hazardous areas | 12 | 1,0 | 6 |
| Structural Fire Protection | Installation and inspection of products for passive fire protection in buildings | 12 | 1,0 | 6 | -- |
| Fire Investigation | Fire Investigation | 30 | 2,5 | 15 | -- |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Egress & Life Safety Analysis | Evacuation Steward | 6 | 0,5 | 3 | No.2: Panic & emergency exit devices  No.5: Guidance signs, Emergency lighting and General lighting  No.19: Fire safety engineering concerning evacuation from buildings  No.33: Evacuation of people with disabilities |
| Management of Wildland-Urban Interface Fires | Risk Management of Natural Hazards | 30 | 2,5 | 15 | No.6: Forest Fires |
| Industrial Fire Safety | Fire Safety in Transformation Facilities | 12 | 1,0 | 6 | No.22: Wind turbines-Fire Protection Guideline  No.14:  Fire protection in information technology facilities  No.18:  Fire & Protection in chemical manufacturing site  No.12:  Fire safety basics for hot work operatives |
| Introduction to thermography | 18 | 1,5 | 9 |
| Thermography of electrical installations | 30 | 2,5 | 15 |
| Hot works | 6 | 0,5 | 3 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Non-Industrial Fire Safety | | Introduction to the Management of Hotel Fire Safety | 6 | 0,5 | 3 | No.29: Protection of paintings: Transport, exhibition and storage  No.30: Managing fire safety in historical buildings |
| Fire Safety and Security Museums and Historical Premises Specialist | 30 | 2,5 | 15 |
| Consequence Analysis | | Risk management of technical safety | 30 | 2,5 | 15 | No.4: Introduction to qualitative fire risk assessment |
| Business continuity planning | 12 | 2,5 | 6 |
| Risk Based Land use planning | | Fire Protection Management System | 6 | 0,5 | 3 | No.1:  Fire protection management system  No.21:  Fire prevention on construction sites |
| Fire Safety During Construction Works | 6 | 0,5 | 3 |
|  | \* Related to Table 1  \*\* Related to Table 2 | | | | | |

Table 4. CFPA-E Courses and Guidelines for “Application Focused” FSE Topics

# Quality and Independency

Quality Control and Independence are of key importance for the development of the certification.

## Internal Audits

This refers to the Internal Audits Procedure for CFPA-E Technical Cycle

## Independency

Only one of the at least three members of the National Examination Board should be personnel of the CFPA member country.

# European guidelines

*Fire (*[*https://cfpa-e.eu/category-guidelines/fire-prevention-and-protection/*](https://cfpa-e.eu/category-guidelines/fire-prevention-and-protection/)*)*

Guideline No 1 F - Internal fire protection control

Guideline No 2 F - Panic & emergency exit devices

Guideline No 3 F - Certification of thermographers

Guideline No 4 F - Introduction to qualitative fire risk assessment

Guideline No 5 F - Guidance signs, emergency lighting and general lighting

Guideline No 6 F - Fire safety in care homes

Guideline No 7 F - Safety distance between waste containers and buildings

*Guideline No 8 F - withdrawn*

Guideline No 9 F - Fire safety in restaurants

Guideline No 10 F - Smoke alarms in the home

Guideline No 11 F - Recommended numbers of fire protection trained staff

Guideline No 12 F - Fire safety basics for hot work operatives

Guideline No 13 F - Fire protection documentation

Guideline No 14 F - Fire protection in information technology facilities

Guideline No 15 F - Fire safety in guest harbours and marinas

Guideline No 16 F - Fire protection in offices

Guideline No 17 F - Fire safety in farm buildings

Guideline No 18 F - Fire protection on chemical manufacturing sites

Guideline No 19 F - Fire safety engineering concerning evacuation from buildings

Guideline No 20 F - Fire safety in camping sites

Guideline No 21 F - Fire prevention on construction sites

Guideline No 22 F - Wind turbines – Fire protection guideline

Guideline No 23 F - Securing the operational readiness of fire control system

Guideline No 24 F - Fire safe homes

Guideline No 25 F - Emergency plan

*Guideline No 26 F - withdrawn*

Guideline No 27 F - Fire safety in apartment buildings

Guideline No 28 F - Fire safety in laboratories

Guideline No 29 F - Protection of paintings: transports, exhibition and storage

Guideline No 30 F - Managing fire safety in historic buildings

Guideline No 31 F - Protection against self-ignition end explosions in handling and storage

of silage and fodder in farms

Guideline No 32 F - Treatment and storage of waste and combustible secondary raw

materials

Guideline No 33 F - Evacuation of people with disabilities

Guideline No 34 F - Fire safety measures with emergency power supply

Guideline No 35 F - Fire safety in warehouses

Guideline No 36 F - Fire prevention in large tents

Guideline No 37 F - Photovoltaic systems: recommendations on loss prevention

Guideline No 38 F - Fire safety recommendations for short-term rental accommodations

Guideline No 37 F - Fire protection in schools

Guideline No 38 F - Fire safety recommendations for short-term rental accommodations

Guideline No 39 F - Fire protection in schools

Guideline No 40 F - Procedure to certify CFPA-E Fire Safety Specialists in Building Design

Guideline No 40 F - Safety instructions for the use and charging of small and medium size lithium ion powered devices

*Natural hazards* [*https://cfpa-e.eu/category-guidelines/natural-hazards/*](https://cfpa-e.eu/category-guidelines/natural-hazards/)*)*

Guideline No 1 N - Protection against flood

Guideline No 2 N - Business resilience – An introduction to protecting your business

Guideline No 3 N - Protection of buildings against wind damage

Guideline No 4 N - Lighting protection

Guideline No 5 N - Managing heavy snow loads on roofs

Guideline No 6 N - Forest fires

Guideline No 7 N - Demountable / Mobile flood protection systems

Guideline No 8 N - Ensuring supplies of firefighting water in extreme weather conditions

Guideline No 9 N - Protection against hail damage

Guideline No 10 N - Heavy rain and flash flood; Recommendations on flood prevention and protection

*Security (*[*https://cfpa-e.eu/category-guidelines/security/*](https://cfpa-e.eu/category-guidelines/security/)*)*

Guideline No 1 S - Arson document

Guideline No 2 S - Protection of empty buildings

Guideline No 3 S - Security systems for empty buildings

Guideline No 4 S - Guidance on keyholder selections and duties

Guideline No 5 S - Security guidelines for museums and showrooms

Guideline No 6 S - Security guidelines emergency exit doors in non-residential premises

Guideline No 7 S - Developing evacuation and salvage plans for works of art and

heritage buildings

Guideline No 8 S - Security in schools

Guideline No 9 S - Recommendation for the control of metal theft

Guideline No 10 S - Protection of business intelligence

Guideline No 11 S - Cyber security for small and medium-sized enterprises

Guideline No 12 S - Security Guidelines for Businesses

Comments and corrective actions:



[**www.cfpa-e.eu**](https://www.cfpa-e.eu)